Collapse All Expand All | Language Filter: Visual Basic Language Filter: C#Language Filter: Visual C++Language Filter: JavaScript Visual Basic C# Visual C++ JavaScript | See Also
.NET Framework Class Library
RemoteEventService..::EventPollingInterval Property

BMXNET 4.0 Developer API

The number of milliseconds (ms) to wait before polling. If a polling event is currently being processed when a second event is trigger, the second event is skipped. It's recommended to keep this interval at 5000 (5 seconds) or higher.

Namespace: IndianHealthService.BMXNet
Assembly: BMXNET40 (in BMXNET40.dll)

# Syntax

| C# |  |  | Visual Basic |  |  | Visual C++ |

    int EventPollingInterval { get; set; }

    Property EventPollingInterval As Integer

    property int EventPollingInterval {
    	int get ();
    	void set (int value);
    }

# See Also

RemoteEventService Interface
IndianHealthService.BMXNet Namespace