English	French	Notes	Complete/Exclude
 filers are running **			
[End of list - total of 			
Outgoing			
Incoming			
Task Number of 			
Asked			
To Stop			
Last Known Date/Time			
Time Difference			
) Start incoming filer  			
) Stop incoming filer  			
) Delete incoming filer			
) Start outgoing filer  			
) Stop outgoing filer  			
) Delete outgoing filer			
) Next 4 lines in list  			
) Back 4 lines in list 			
Type selection: 			
Qq^			
filer task number			
Outgoing 			
Incoming 			
filer is no longer defined **			
filer has not started yet			
filer stopped but didn't delete itself			
filer has not been [re]scheduled **			
filer has stopped due to error **			
Response must be a number between 			
Enter '??' to see a list of valid selections			
Valid Selections: 			
 is not a valid selection			
Valid pointer to Message Text file (#772) not passed			
Could not determine parent message			
Could not determine sending application			
Could not determine receiving application			
Message Type Undefined for protocol 			
Missing Processing ID Site Parameter.			
-1^No parent			
-1^No server for this node			
-1^No client for this node			
MType undefined for protocol 			
Valid pointer to Message Administration file (#772) not passed			
Missing processing ID Site parameter.			
by reference			
HLCSHDR3 			
HLCSHDR3 DEBUG			
Debug data created by DEBUG~HLCSHDR4			
Enter 773 IEN: 			
  no debug data found...			
Original (91)			
Array (90)			
MSH-Segment			
snd app			
snd fac			
rec app			
rec fac			
HL7 Protocol Messaging Fields			
This 'HL7 Protocol Messaging Fields' report holds information that will help			
you determine the effects from changes to routing-related fields in the MSH			
segment when messages are sent between or within VistA HL7 systems.			
Additional explanation is included at the bottom of the report.			
Press RETURN for 'printout help', or '^' to exit... 			
Press RETURN to exit... 			
The original MSH segment is...			
The MSH segment, after modification by passed-in data, is...			
SENDING APPLICATION			
SENDING FACILITY			
RECEIVING APPLICATION			
Before your changes above, the modified MSH segment was...			
After your changes, the MSH segment is...			
Message being sent...			
Protocol-derived value of 			
Passed-in value of 			
Enter new value for 			
No changes will be made...			
The variable 			
 will be changed to '			
This value will be stored in the 			
field in the MSH segment...			
The MSH segment was not changed...			
   changed to...			
You have made some changes to the original MSH segment.  Do you want to			
 these changes, and reset the MSH segment to it's original state?			
Reset MSH segment			
Enter ACTION			
MSH Segment Values			
Variable			
Value			
Enter FIELD #: 			
Current '			
Field value			
  nothing changed...			
SND-APP			
REC-APP			
ORU~R01			
Enter ERROR REASON: 			
MSH: 			
Press RETURN to mark errored, or enter '^' to abort... 			
  no action taken...			
Marking 772's #			
Aborted!! 			
Marking 773's #			
HLCSHDR5 ERR			
No ^TMP(			
,$J) data exists...			
The entries in ^TMP(			
,$J) will be marked in error now.			
Press RETURN to start error marking... 			
Error Marking Utility			
HL7-AC			
IN QUEUE FRONT POINTER			
HLmgr:			
Link Manager already running!			
Would you like to stop the Link Manager now			
Link Manager is NOT currently running!			
Would you like to start the Link Manager now			
Link Manager has been asked to stop			
HL7 Link Manager			
Link Manager queued as task number 			
Unable to start/restart Link Manager			
HL7 Logical Link 			
 shutdown due to TaskMan unable to process task request			
This option is used to launch the lower level protocol for the			
appropriate device.  Please select the node with which you want			
to communicate			
A Lower Layer Protocol must be selected before start-up can occur.			
No routine has been specified for this LLP.			
This LLP is a multi-threaded server. It is controlled by external service, i.e. TCPIP/UCX. You must use the external service to start this LLP.			
The LLP was last started on 			
The LLP was last shutdown on 			
The LLP appears to be online already !			
NOTE: The lower level protocol for this application is already running.			
This LLP is already enabled!			
Unable to enable this LLP !			
This LLP has been enabled!			
This LLP will start on node 			
 if it is run in the Background.			
Method for running the receiver			
Enter F for Foreground (and trace)			
      B for Background (normal) or			
      Q to quit without starting the receiver			
Job was queued as 			
Unable to queue job.			
-Unable to Open the Device !			
Check that Port is Logged Out, and that the			
Lower Level Protocol is not Already Running.			
This option is used to shut down the lower level protocol for the			
appropriate device.  Please select the link which you would			
like to shutdown.			
The lower level protocol is already 			
The lower level protocol was started on 			
Okay to shut down this job			
The job will not be shut down.			
Unable to shutdown logical link!!!			
The job for the 			
 Lower Level Protocol will be shut down.			
HL7 Msg 			
ADDR FLAGS			
HL7 Logical Link: 			
Error handing HL7 message off to Mailman			
Type 'Q' to quit: 			
Incoming filers running => 			
Outgoing filers running => 			
Select a Command:			
(N)EXT  (B)ACKUP  (A)LL LINKS  (S)CREENED  (V)IEWS  (Q)UIT  (?) HELP: 			
Vv			
CANNOT 			
 BEYOND END OF BUFFER			
IN QUEUE BACK POINTER			
OUT QUEUE BACK POINTER			
OUT QUEUE FRONT POINTER			
You have the following options when monitoring the Messaging System:			
Enter the command letter parentheses: N,B,Q,A,S,V or ?			
(N) takes you to the next page of the display of Logical Links.			
(B) takes you back one page.			
(Q) terminates the monitor.			
(A) provides a display of all links defined on your system.			
(S) displays only those links that have had message traffic.			
(V) prompts for a view name and displays links defined in view.			
    Note that (S) is the default display at startup.			
**PRESS <RET> TO CONTINUE**			
Device Types and corresponding prefixes:			
PC -- Persistent TCP/IP Client			
NC -- Non-Persistent TCP/IP Client			
SS -- Single-threaded TCP/IP Server			
MS -- Multi-threaded TCP/IP Server			
SH -- Serial HLLP			
SX -- Serial X3.28			
MM -- MailMan			
Editing of logical link data is occurring right now.  For this reason, some of			
the information on the 'System Link Monitor' report might not be accurate for			
the following node(s)...			
Press RETURN to print report or '^' to exit... 			
Zero			
***TASKMAN NOT RUNNING!!!***			
TaskMan running 			
***LINK MANAGER NOT RUNNING!!!***			
Link Manager running			
Queue: 			
     Message number: 			
     Message status: 			
     Message error: 			
     Message text:			
HL7 LOGICAL LINK INFORMATION			
No data found for this request			
Select HL7 Logical Link: 			
All Links			
Select queue for report			
ALL:ALL ERRORS;F:FINISH SELECTING ERRORS			
Select an error code to sort by			
Select the list of errors that you would like to sort by.  There are also			
two special selections.  ALL means that you would like to sort on all the			
error codes.  F means that you have finished selecting error codes.			
ALL:ALL STATUS;F:FINISH SELECTING STATUS CODES			
Select a status code to sort by			
Select a status code to sort the report by.  There are two special			
selections.  ALL indicates you would like a report on all the statuses.  The			
F means you are finished selecting statuses.			
HL7 LOGICAL LINK REPORT			
Logical Link not available			
Parent Message not available			
Message Type (field #772,14) Error			
Awaiting Ack			
-1^Queue not given			
-1^Invalid queue			
-1^Invalid Direction			
Stub			
-1^NO NEXT RECORD			
-1^Internal Entry Number missing			
-1^Invalid IEN			
-1^Invalid direction			
-1^No message number			
Select the IN queue or OUT queue (relative to DHCP)			
Select queue			
Select if you want to EDIT or CREATE and entry in a queue			
CREATE or EDIT entry			
Editing entry number: 			
No Entries in this Queue !			
Re-queue these messages?			
 to re-queue, or 			
 to quit without re-queueing.			
HL MESSAGE REQUEUER - 1			
Known Logical Links			
** No logical links have been defined **			
HL MESSAGE REQUEUER - 2			
Processed Messages in Logical Link 			
** There are no entries in this queue **			
 ===>> Screen Attributes NOT Defined. Use ^ZU or ^XUP before invoking.			
 ===>>>  NO MATCHING RECORDS  <<<=== 			
DI*21.0*32			
MESSAGE TEXT			
IEN RECORD #   MESSAGE ID #         Log Link   Msg:Evn IO Sndg Apl Rcvr Apl HDR			
Search Transmission Log			
Start/Stop Time Selection			
  Enter START Date and Time. Date is required.			
  Enter END Date and Time. Date is required.			
Enter Record Number: 			
  ==>  NO SUCH RECORD NUMBER <== 			
DATE AND TIME ARE BOTH REQUIRED			
IORVON;IORVOFF;IOINHI;IOINLOW			
 . . . PLEASE WAIT, THIS CAN TAKE AWHILE . . .			
MESSAGE ID #         D/T Entered   Log Link   Msg:Evn IO Sndg Apl Rcvr Apl     			
Logical Link Selection			
Select Logical Link:  ALL//			
 NOT VALID 			
 Fake Record to pass Browser edits. 			
Record #: 			
Message #: 			
Logical Link: 			
Ack To MSG#: 			
ERR MSG: 			
ERR TYPE: 			
Sending Appl: 			
Receiving Appl: 			
Message Type: 			
Event Type: 			
MESSAGE HEADER: 			
MESSAGE TEXT: 			
#773-IEN      Message-ID       Procd     Log-Link   Msg:Evn IO Sndg-Apl Rcvr-Apl			
Error Type Selection			
Select Error Type:  ALL//			
PLEASE WAIT, THIS CAN TAKE AWHILE...			
IEN Record #   MESSAGE ID #         Log Link   Msg:Evn IO Sndg Apl Rcvr Apl			
 No Header in MSG Admin File (#773)			
 No Message in MSG Text File (#772)			
Select Logical Link for Report:  ALL//			
Message/Event Type Search			
Select Message Type for Report:  ALL//			
Select Event Type for Report:  ALL//			
Message Criteria for Search			
Select Status Code for Report:  ALL//			
   If you answer NO below, you will be allowed to specify the number of			
   errors to be included in the report.			
Print all errors			
   All errors in the date range you specify next will be included			
   in the report.			
   The newest 			
 errors, for every error status, in the date range you			
   specify next will be included in the report.			
The first entry at your site is from 			
Enter START DATE/TIME			
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
