English	French	Notes	Complete/Exclude
Terminate license now			
Keep license and extend time			
Defaulting 'NOW + 7 days' below...			
Enter CUTOFF DATE			
Enter a future  cutoff date/time now after which no remote requests by			
non-VistA HL7 team message recipients will be honored.			
  enter time one hour or more in future...			
Select ACTION			
Enter NEW CUTOFF DATE/TIME			
The current license has been changed to 			
Enter the email address of the recipient(s).  (Enter the address of an			
existing user and they will be removed.)			
Hint:			
You may enter 			
 that is less exact than the complete			
email address and not compromise security.  For example, if			
the remote requester is named 'John Doe' and will be sending			
requests from the Buffalo VAMC, you still might not know			
the exact email address to enter.  (E.g., Should you enter			
is why it is often advantageous to enter something like			
'DOE@BUFFALO' and also 'DOE@MED.VA.GOV'.  When a remote 			
request is received, as long as 'DOE' is in the sender's			
name, and either 'BUFFALO' or 'MED.VA.GOV' is in the			
address, it will be honored.			
Enter REMOTE ADDRESS			
No action taken! (Use 'NAME@ADDRESS' format.)			
Warning!!			
  The current license, along with all licensed requesters, will			
                   be deleted if you continue.			
License '			
' will be used after you enter cutoff date...			
No license exists...			
If you cancel license, the code and all requesters will be removed!			
OK to cancel license			
  license canceled...			
requester unknown.			
no license exists.			
the current license has expired.			
incorrect code received.			
Requester is not licensed.			
Request# 			
Refused (			
HL7 Remote Request Refusal: 			
HOLD(			
The following remote request for VistA HL7 data has been refused.			
Details are included below.			
---------------- editing entry ----------------			
Event Monitoring System Enter/Edit			
fires off			
This '			
' menu option			
is not yet implemented.			
Press RETURN to return to menu...			
The most recent 772 IEN is... 			
Stop entering 772 IENs			
  no entries selected...			
Stop entering recipients			
Enter RECIPIENT			
No recipients were entered.  You may just display the data on-screen.			
Display to screen			
Press RETURN to send message, or '^' to exit... 			
Requested 772#: 			
 Requested Data 			
HL7 Data - 			
no msg sent...			
Enter 772 IEN			
Send File 772 & 773 Data to Remote Recipient(s)			
List of problems			
Problem          totals			
Logical Link Display			
What information for IN and OUT QUEUEs do you want to see?			
1  Show IENs			
2  Show Summary nodes			
5  Find skips			
6  Message date search			
Totaling...			
End of output... 			
IN QUEUE F			
IN QUEUE B			
OUT QUEUE F			
OUT QUEUE B			
Select LINK: 			
Links with queues			
Link			
IQ Totals			
OQ Totals			
Mail]			
Mail^HLLP^X3.28^TCP			
First IEN = 			
 Last IEN = 			
Enter IEN			
Select QUEUE			
Just completed a search using a starting point of IEN=			
, and an offset			
.  You may now enter a new starting IEN and offset.			
Enter OFFSET: 			
Monitor Test Utility			
This utility sets the ^TMP(			
,$J) node to 			
 to avoid any			
Event Monitor activity.  This enables the debugging of M code.			
   no M code found...			
You may ZG 			
DO the MCODE			
OK to test now			
   no action taken...			
ZG 			
... some data not shown ...			
HLEVUTI1 			
M Code Requeue Utility			
No M Code API run data exists...			
Task#			
Next task#			
Queue time			
OK to queue job			
  job not started...			
Queued to task# 			
HLEVUTI2-Queued Jobs			
HLRUNS*			
HLEVREQ-			
Event Monitor HLEVUTI2 Requeue			
END OF QUEUING			
Line of text saved by SAVE(TXT).			
Enter TAG~ROUTINE			
Enter the M code API to be called by background jobs.  Enter it in the format			
'TAG~ROUTINE'.  (Use the tilde (~) character in place of the up-arrow.)			
Enter STOP TIME: 			
Enter a future date/time up to 			
New jobs will be requeued until the date/time you enter now.  You cannot queue			
jobs past seven days in the future.			
Date/time you enter must not be in the past...			
Enter REQUEUE FREQUENCY (min)			
New jobs will be requeued for the number of 'requeue frequency' minutes			
in the future you specify now.			
The queuing of jobs to 			
 has finished.  #			
 jobs were queued.			
Task#         Start        Finish			
Data in ^XTMP(			
No data exists... 			
Existing M code job run data...			
Started: 			
    Job still running!!			
OK to delete ALL M Code requeue data			
  nothing deleted...			
Killing ^XTMP(			
File 772 & 773 IEN Display			
This API displays the last internal entry number (IEN) in the following files:			
  * HL Message Text file (#772).			
  * HL Message Administration file (#773).			
The last IEN in these files are recollected and redisplayed every 15 seconds.			
After every display of these IENs, you may take the following actions:			
  * Do nothing, & the information will be redisplayed in 15 seconds.			
    (You may change the refresh seconds by entering a number of seconds			
    and pressing RETURN.)			
  * Hit return to force information redisplay.			
  * Enter an uparrow ('^') and press RETURN to exit.			
Press RETURN to start, or '^' to exit... 			
LAST-772-IEN			
LAST-773-IEN			
Monitor 			
Monitor current			
Monitor current [next job 			
HLEV-			
Aborted by installation pre-init.			
pointed to			
Purges: 			
 master jobs.  			
Purging of 776 and 776.2 (non-setup) Data			
There is no data to delete...			
No data to delete for file 			
OK to delete file 			
 ... not deleted ...			
Official VistA HL7 Event Monitor Code			
HLEV REP			
HLEV STUB 			
HLEV Stub Record Search			
IEN [			
Run site:  			
Some stub entries exist in the HL Logical Link file (#870) that			
appear to be 			
.  Someone at the site needs to check out			
and possibly change their status to DONE.			
Link          In/Out     IENs			
hangs around			
Exiting... 			
No link selected.  Start again... 			
No stub entry exists for link.			
Stub record# 			
 found.  It's status is about to be changed to DONE...			
OK to correct			
Press RETURN to continue searching... 			
Select the QUEUE to search			
Select LOGICAL LINK: 			
Searching for stub records...			
Stub Record Correction			
Mother			
Mother of All			
# job runs last 24 hours			
PARM STOP			
STOP REQUESTED			
JOB ABORTED			
TOO EARLY			
Last master job run			
Next master job at			
Recent Event Runs			
Event-Name                      Run#1          Run#2          Run#3			
 (Dates in [brackets] are still running.)			
HLEV CHK773AC 			
VistA HL7 773 AC Xref Check			
Task# 			
HLEV CHK773AC			
CHECKAC-3			
No 870			
AC-NO 870			
No 773			
AC-NO 773			
Proc'd			
AC-PROC'D			
hang around			
Hung#			
AC-HUNG			
 Problem AC Entry 			
 Entry After AC Problem 			
COMING  			
GOING  			
Protocol Disabled			
MTN_ETN			
Invalid Subscriber Protocol			
Subscriber Application Missing in Protocol File			
'HL INTERFACE WORKBENCH - 1' List Template...			
HL INTERFACE WORKBENCH - 1			
HL INTERFACE WORKBENCH - 1^1^^80^5^17^1^1^Tool^HL DT/IW MENU - SCREEN 1^HL-7 Interface Workbench^1^^1			
IW-SCRN1			
'HL INTERFACE WORKBENCH - 2' List Template...			
HL INTERFACE WORKBENCH - 2			
HL INTERFACE WORKBENCH - 2^1^^80^5^17^1^1^Tool^HL DT/IW MENU - SCREEN 2^HL-7 Interface Workbench^1^^1			
IW-SCRN2			
'HL INTERFACE WORKBENCH - 3' List Template...			
HL INTERFACE WORKBENCH - 3			
HL INTERFACE WORKBENCH - 3^1^^80^5^17^1^1^Tool^HL DT/IW MENU - SCREEN 3^HL-7 Interface Workbench^1^^1			
IW-SCRN3			
'HL INTERFACE WORKBENCH - 4' List Template...			
HL INTERFACE WORKBENCH - 4			
HL INTERFACE WORKBENCH - 4^1^^80^5^17^1^1^Tool^HL DT/IW MENU - SCREEN 4^HL-7 Interface Workbench^1^^1			
IW-SCRN4			
'HL INTERFACE WORKBENCH - 5' List Template...			
HL INTERFACE WORKBENCH - 5			
HL INTERFACE WORKBENCH - 5^1^^80^5^17^1^1^Tool^HL DT/IW MENU - SCREEN 5^HL-7 Interface Workbench^1^^1			
IW-SCRN5			
'HL MESSAGE REQUEUER - 1' List Template...			
HL MESSAGE REQUEUER - 1^2^^80^5^18^1^1^^^HL7 Message Requeuer^1^^1			
'HL MESSAGE REQUEUER - 2' List Template...			
HL MESSAGE REQUEUER - 2^1^^80^5^18^1^1^^HL CS/RQ MENU - SCREEN 2^HL7 Message Requeuer^1^^1			
'HL MESSAGE REQUEUER - 3' List Template...			
HL MESSAGE REQUEUER - 3^2^^240^5^18^1^1^^^HL7 Message Requeuer^1^^1			
HL LOG 			
Log data created by call to HLLOG			
NULL DEVICE			
No pointer to Message file(#3.9)			
No message found at #			
 in Message file(#3.9)			
No message contents at #			
Lower Level Protocol Error - 			
Checksum			
Character Count			
 Did Not Match			
BHS,MSH			
Application Level error - Header Segment Missing			
 at GENERATE^HLMA entry point			
Missing IP Address			
PING worked			
Incorrect response			
-1^Error during read			
-1^Error during write			
Calling DNS			
Domain Unknown			
Domain, 			
Port: 			
DNS Returned: 			
Trying 			
-1^DNS Lookup Failed			
 at GENACK^HLMA1 entry point			
 at SEND^HLMA entry point			
MTYPE_EVENT			
 in HLCSHDR1			
HLEV INSTALL 			
HLEV INSTALLATION MONITOR LIST			
The installation of the Event Monitoring software held in patch			
HL*1.6*109 is complete. 			
HLEV INSTALL 9999999.99999			
HL*1.6*109 Installation - Site# 			
Setup instructions message #			
STUB 870 SEARCH			
XREF CHECK - FILE 772 & 773			
HLEV INSTALL 9999999.999999999			
HLEV INSTALL			
.08///HEALTH LEVEL SEVEN			
 - New and changed monitors.			
Monitors changed during installation			
New monitors			
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
