English	French	Notes	Complete/Exclude
Z SEGMENT is null			
MFI CODE is null			
PRE-UPDATE ROUTINE is null			
POST-UPDATE ROUTINE is null			
MAIL GROUP is null			
MFE ID & ALT ID field and codsys required			
MFE PKV X-REF required			
MFE PKV types are null			
ASSIGNING AUTHORITY is null			
 is pointer EXTENDED POINTER LKUP is NULL			
 missing FIELD NUMBER			
 MULT IEN FUNCTION is null			
 SUBFILE KEY LKUP/KEY SEQ mismatch			
 SUBFILE null with subfile parameters			
XUMF get 			
 using MFS			
1IFN not valid MFS in XUMF			
1IEN not valid MFS in XUMF			
1type not support by MFS in XUMF			
XUMF MFR^XUMF 			
XUMF MFQ			
XUMF MFS			
XUMF Load DOD DMIS ID's			
XUMF ARRAY			
XUMF IMF EDIT STATUS			
XUMF LOAD INSTITUTION			
Patch XU*8*335 clean 4.1 and 4			
XUMF333 clean 4.1 and 4			
HEALTH CARE SYSTEM			
DUZ not defined.  Please log on.			
MISSING DATA - please fix			
 is okay			
 is MISSING DATA - please fix			
IEN null			
STATE is missing			
Physical address St. line 1 missing			
Physical address City missing			
Physical address ZIP missing			
Physical address St. line 2 missing			
Mailing address St. line 1 missing			
Mailing address City missing			
Mailing address State missing			
Mailing address ZIP missing			
Mailing address St. line 2 missing			
FACILITY TYPE is missing			
FACILITY TYPE is not NATIONAL			
OFFICIAL VA NAME is missing			
Inactive facility NAME not ZZ'd			
XUMF 4.1			
...getting Facility Types - wait please 5 min...			
...getting Institutions - wait please 10 min...			
...connecting with master file server...			
Connection to master file server failed!			
XUMF NAME			
No duplicates to select from!			
Pointed to by HL7 Logical Link			
*select other entry*			
XUMF 			
XUMF DSTA			
XUMF TMP			
INSTITUTION NAME			
***No duplicates***			
This action will auto-delete local/duplicate station numbers.			
deleting duplicate station number 			
 from IEN: 			
deleting local station number 			
XUMF LLCL			
FACILITY TYPE			
***None found***			
XUMF NATL			
NATIONAL NAME			
XUMF TABLE			
GOLD NAME			
...getting FACILITY TYPE file...			
...getting INSTITUTION file...			
...please wait...(approx. 5 minutes)...			
IFR clean up			
XUMF INSTITUTION			
Duplicates sta #s exist! -- NOTHING UPDATED!!!			
XUMF CHCK			
Local/Duplicate station #s exist -- use DSTA			
INSTITUTION file not updated with NATIONAL data -- use AUTO			
CONGRATULATIONS!!!  Update complete!			
This list displays duplicate STATION NUMBER (#99).			
The action associated with this list will automatically			
remove the value from field #99 for local and duplicate			
This list displays entries that are in the INSTITUTION (#4)			
file but not in the national file.			
This list is informational only and has no actions associated			
with it.			
This list displays the Master Institutution File data.			
This list displays station numbers that are in the national			
file but not in the INSTITUTION (#4) file.			
This action will automatically update the INSTITUTION (#4) file			
with national data.			
Use this action to check if the all the required steps have			
been performed and the clean up has completed.			
This main screen displays a side-by-side view of the INSTITUTION			
(#4) file and the national file names by station number.			
LLCL - lists local station numbers to be deleted.			
DSTA - automatically deletes local/duplicate station numbers.			
NATL - lists Institution Master File entries to merge.			
AUTO - merges national data with local INSTITUTION (#4) file.			
CHCK - run this action to see pending clean up actions to perform.			
XUMF Institution file background cleanup			
XUMF ADD			
XUMF MOD			
XUMF DEL			
VETERANS INTEGRATED SERVICE NETWORK			
VISN 23			
A check of the INSTITUTION file (#4) indicates the IFR			
cleanup has NOT been performed.			
The IFR cleanup is a required action.  Future initiatives			
are dependant on consistent and reliable Institution data			
at each site.  A copy of this message is being sent to NVS			
for tracking purposes.			
If you require assistance performing the IFR cleanup,			
you may contact NVS and someone will contact you and			
help you with the IFR cleanup process.  To request			
assistance you may send a MailMan message to the			
G.XUMF INSTITUTION mail group on FORUM or log a NOIS.			
Note: Running the IFR cleanup on LEGACY systems is			
OPTIONAL.  If this message refers to a legacy system			
please disregard this message.			
IFR/cleanup/REQUIRED at 			
G.XUMF INSTITUTION			
G.XUMF INSTITUTION@FORUM			
~FACILITY TYPE~VA			
A backgroud job just updated your Institution file			
with data from the Institution Master File (IMF)			
on FORUM.			
This job was a special task to insure sites that			
have already run the cleanup are up-to-date with			
all updates.			
These updates were broadcast previously, but your			
site may not have received them due to enabling			
and/or disabling broadcasting to sites for various			
This message has three sections (in addition to this			
initial text.)  The first section lists entries that			
have been added to your file.  The second section			
lists existing entries that have modified.  The third			
section lists entries that have had their STATUS (#11)			
changed from National to Local and their STATION			
NUMBER (#99) removed (was never a valid sta #.)			
The lists are in Station Number order and are up-arrow			
delimited strings in the HL7 Institution segment			
format.  The values correspond to the FileMan fields			
SECTION ONE			
The following entries were ADDED:			
None.			
SECTION TWO			
The following entries were MODIFIED (old/new value):			
SECTION THREE			
The following STATION NUMBERS were removed:			
Note: Just the STATION NUMBER (#99) was removed			
and the STATUS (#11) changed to Local.  The entry			
itself was NOT deleted.			
IFR/cleanup/updates at 			
Station numbers added: 			
File entries modified: 			
IFR/cleanup/status at 			
UPDATE FILE			
XUMF MFN			
Are you ready to update the Institution Master File			
WARNING: You modified your entry without updating the IMF!			
...send HL7 message to Master File Server...			
XUMF IMF MFK^XUMF 			
XUMF IMF MFN			
Sent.			
Enter Station Number			
   Invalid selection!			
 to edit an inactive faciliy log on to that division			
 you must have DIVISION in your NEW PERSON multiple.			
 If Inactive facility not selectable - assign with			
 XUMGR security key.			
Enter VISN Number			
Parent ASSOCIATION - Enter the admin PARENT for this facility			
QRD,QDT,QFC,QP,QID,DRT,DRDT,QLR,WHO,WHAT,WDDC,WDCVQ,QRL			
MFE segment NULL key 			
MFE segment couldn't resolve IEN			
update DIE call error message in ZZZ			
file DIE call error message in ZZZ			
update DIE call error message in SUBFILE			
Null KEY found in the following segment: 			
HL7 message ID: 			
MFS ERROR			
G.XUMF ERROR			
DINUMed field cannot			
MSA segement error/reject message			
XUMF Broadcast IMF address changes			
IMF HANDLER ERROR MESSAGE			
A XUMF ID			
XUMF MFK^			
IEN ARRAY			
VA FM			
INFORMATION INFRASTRUCTURE			
VA TS			
XUMF PRE			
PRE UPDATE VALUES:			
POST UPDATE VALUES:			
MFS UPDATE - 			
G.XUMF SERVER			
XUOAA PMU			
EMAIL ADDRESS			
CURRENT DEGREE LEVEL:ABBREVIATION			
PROGRAM OF STUDY			
LAST TRAINING YEAR			
msgid^error code^error msg			
Clinical Trainee Core Dataset			
Clinical Trainee Transmission Count			
Number of trainees transmitted to OAA: 			
XUOAA CLIN TRAINEE TRANS			
G.XUOAA CLIN TRAINEE TRANS			
Setting up programmer environment			
Switched Identities			
HOME;			
Terminal Type set to: 			
 new message			
XUS-XUP SET ERROR TRAP			
XUS-XUP VPE			
Access Code			
Want to record the error: No// 			
Site Honolulu - no action taken.			
Unable to lookup protocol 'XUHUI FIELD CHANGE EVENT' - no action taken.			
2///*Do NOT remove this message			
Protocol 'XUHUI FIELD CHANGE EVENT' has been DISABLED.			
XUHUI SEND MESSAGE			
Unable to lookup protocol 'XUHUI SEND MESSAGE' - no action taken.			
Protocol 'XUHUI SEND MESSAGE' has been DISABLED.			
This option will print a 			
 report which will display the System Response			
Time (RT) hourly averages over a selected range of dates.  The data that is 			
displayed in this report is from the data that is stored in the ^%ZRTL(3			
global node.			
This report should be printed to a 132 column output device.			
System Response Time Report for 			
This report will print a System Response Time (RT) bar graph of hourly			
averages over a selected range of dates.  The data that is displayed in			
this report is from the data that is stored in the ^%ZRTL(3 global node.			
Enter Starting Hour			
Ending Hour			
GRAPHIC RESPONSE TIME REPORT			
RESPONSE TIME LOG for VOLUME SET: 			
ROUTINE: 			
AVE RESPONSE TIME SECONDS for DATES 			
REMARKS:<< 			
 sample(s) greater than 			
 seconds; not included in average >>			
 sample(s) equal to 0 seconds >>			
This report will print a report which will display the System Response			
Time (RT) multiday hourly averages over a selected range of dates.  The			
data that is displayed in this report is from the data that is stored in			
the ^%ZRTL(3 global node.			
MULTIDAY RESPONSE TIME REPORT			
Multiday Average Response Time Log for Volume Set 			
Printed  			
This option will purge all of the System Response Time (RT) metrics in the			
RESPONSE TIME (#3.091), RT DATE_UCI,VOL (#3.092) and RT RAWDATA (#3.094)			
files.  The data in these files is irrecoverable after being purged.			
Purge ALL data in three files			
RESPONSE TIME^3.091P^^			
RT DATE_UCI,VOL^3.092^^			
RT RAWDATA^3.094D^0^0			
All of the data in the RT RAWDATA (#3.094) has been purged.			
** THIS REQUIRES VAX DSM **			
Enter the appropriate DSM ENVIRONMENT MANAGER: 			
Press return if logged in as your DSM MANAGER.			
Otherwise, enter the account manager's name.			
DSM/E=			
DSM 			
RTSAMP_			
Select HFS-type DEVICE: 			
$!SCRIPT DRIVER-SUBMIT TO BATCH			
$ SET ON			
$ ON ERROR THEN GOTO EXIT			
$ ENV MAIL^XURTL4			
$ PURGE RTSAMP*.*			
...Done. The command file, 			
SUBMIT/NOPRINT/KEEP 			
TEXT FROM RT SAMPLER			
XRTLTXT($J,			
RTSAMP.			
-AUTO RESPONSE TIME SAMPLER			
RESPONSE TIME INFO ON NODE 			
This option queues a task to copy the Response Time (RT) data that is stored			
in the ^%ZRTL(3 global node to the RT RAWDATA (#3.094) file.  When significant			
amounts of RT data are involved, this option will take a long time for			
completion and can consume a lot of disk storage.  It will TRIPLE the size			
of the ^%ZRTL global in MGR where the Response Time (RT) raw data and files			
are stored.			
COPY %ZRTL DATA TO RT RAWDATA FILE			
Option queued successfully as Task #			
This option will queue a background job that will save the Means into the			
RESPONSE TIME (#3.091) file.  The background job will also purge the			
System Response Time (RT) raw data which is stored in the ^%ZRTL(3 global			
If this option is scheduled to run nightly through TaskManager, the			
default purge through date will be T-1.			
Purge through Date: 			
STORE AND PURGE RT DATA			
ERROR: TaskManager was not able to queue this option.			
Volume set: 			
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
####################	####################	####################	
